TECHNICAL SPECIFICATION

Builder	: Nam Cheong Dockyard Sdn Bhd, Miri, Sarawak
Port of Registry	: Port Kelang	Hull No.	: NC 532
Designer Classification	Year Built : Conan Wu & Associates Pte Ltd Flag : American Bureau Of Shipping (ABS + A1 + AMS Ⓔ FiFi 1 / Towing Vessel)	: January 2008 : Malaysian

PRINCIPAL PARTICULARS	MACHINERY / PROPULSION
Length O.A. Beam Moulded Depth Moulded	: : :	64.80 M 16.00 M 6.50 M	Main Engines Propulsion	: :	2 x Diesel engine Rolls Royce/Bergen 2 x 4500 p.s @ 750 rpm c/w CPP or 4500 BHP each Reduction gear
Gross Tonnage	:	2144 approx.	Performance Speed (Designed)	:	14.0 knots at 100% MCR
Net Tonnage	:	643 approx.	Bow Thruster / Stern Thruster	:	1 x Ulstein CPP type 10 Tons Tunnel Thruster for bow & sterin
Free Deck Space	:	435 m2 approx.	Retractable Thruster	:	1 x 12 tons Ulstein Retractable Thruster
Deadweight	:	1800 tons @ 5.5m draft	Bollard Pull	:	110 tons @ 100% MCR
Generators	:	2 x 405kW Diesel engine, 415/3/50
Steering Gear	:	2 x Independent electro-hydraulic system
Shaft Alternator	:	2 x 1250 kW, 415/3/50

CARGO / TANK CAPACITY	DECK MACHINERY AND TOWING / ANCHOR HANDLING EQUIPMENT
Fresh Water Tank Fresh/Drill Water/SWB Tank	: :	357 m³ approx. 299 m³ approx	Towing & Anchor handling Winch	:	Double Drum Waterfall type @ electro hydraulic system
Fuel Oil Tank	:	523 m³ approx	Tow Drum/Work Capacity	2 x 1500m x 64mm dia.
Liquid Mud/Brine Water Tank Hydraulic Oil Tank	: :	350 m³ approx. 7.50 m³ approx.	Winch Load Capacity	:	250 Tons @ 8.5m/min. at low speed 1st layer
Foam Tank	:	16.00 m³ approx.	Brake Holding	:	300 Tons Brake Holding
Dispersant Lub Oil Storage Tank Dirty Oil Tank	: : :	16.00 m³ approx. 14.50 m³ approx. 4.50 m³ approx.	Storage Reel Winch Capacity Shark Jaw / Towing Pins	: :	1 x 1800 m x 64mm dia. 1 x 300 Tons/160 Tons @ electro hydraulic system
Cement Tank	:	7600 cu. ft. approx.	Stern Roller	:	4.80m (L) x 2.0m dia.
Sewage Holding Tank	:	15.50 m³ approx.	Anchor Windlass/Towing Winch	:	1 x 11 Tons @ electro hydraulic system
Bilge	:	7.40 m³ approx.	Capstan	:	2 x 9 Tons (410mm dia) approx.
Brine /DW/WB Fuel Oil Day Tank	: :	350 m³ approx. 33 m³ approx.	Tugger Winch	:	2 x 10 Tons @ electro hydraulic system
Fresh Water/Drill Water	:	132 m³ approx.

FIRE FIGHTING EQUIPMENT	NAVIGATION / COMMUNICATION EQUIPMENT
External	:	FiFi 1 System @ 2 x 1200 cu. m/hr water monitor c/w deck	GMDSS Radio A3 GPS Navigator	: :	1 complete set 1 unit
spray system	Echo Sounder	:	1 unit
Radar	:	2 units
Internal	:	Complies to classification	Gyro Compass c/w Autopilot	:	1 unit
Society & Solas requirement	Speed Log	:	1 unit
Navtex Receiver	:	1 unit
Automatic Identification System DP-2 System	: :	1 unit 1 set

LIFE SAVING EQUIPMENT
Life raft	:	2 x 10 men and 4 x 25 men	First Aid Kit	:	4 x 25 men
Lifebuoys	:	9 nos. of Perry buoy type	Work Vest	:	8 Driclad type 1
Lifejackets	:	44 nos. Lifejackets	Man Overboard Smoke	:	2 pcs
Oxygen Resuscitator	:	1 set c/w oxygen cylinders & 2 spare bottles	Stretcher	:	1 paraguard rescue stretcher MK3 & 4 points lifting sling
Rescue / Workboats	:	1 x semi rigid type (Zodiac)	Splints	:	6 sets
Pyrotechnics	:	1 x line throwing apparatus 12 parachute distress rockets 2 orange smoke signals

ACCOMMODATION
2 x 1-Man Cabins (2)	4 x 2-Men Cabins (10)	7 x 4-Men Cabins (16)	Total = 38 men
FULLY AIR-CONDITIONED